void setup() {

// initialize digital pin 13 as an output.

pinMode(13, OUTPUT);

}

void loop() {

digitalWrite(13, HIGH); // turn the LED on (HIGH is the voltage level)

delay(1000); // wait for a second

digitalWrite(13, LOW); // turn the LED off by

making the voltage LOW

delay(1000); // wait for a second

}